(2020-01-04 15:59:03):检索到一个驱动器连接:①串口号:COM51
②波特率:57600
③设备ID号:1
当前MODBUS协议32bit数据传输顺序为低16位在前，高16位在后，下载参数时请注意!

(2020-01-04 15:59:03):驱动器当前软件版本信息: 00000001, 设置数据库为 IS650P_V1.2.mdb ;

(2020-01-04 15:59:04):IS_OPERA 初始化成功.

(2020-07-09 11:31:41):IS_OPERA ?????.

(2020-07-09 11:31:41):??1?????;

(2020-07-09 11:33:35):??1?????;

(2020-07-09 11:33:35):IS_OPERA ?????.

(2020-07-09 11:47:13):Not found

(2020-07-09 11:47:14):Not found

(2020-07-09 11:57:10):Not found

(2020-07-09 11:57:12):Not found

(2020-07-09 12:22:19):Not found

(2020-07-09 12:22:20):Not found

(2020-07-09 13:00:30):Not found

(2020-07-09 13:00:30):Not found

(2020-07-09 13:01:14):Serial port 1 is not connected to the device.

(2020-07-09 13:01:14):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-07-09 13:01:16):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-07-09 13:01:16):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-07-09 13:01:17):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-07-09 13:01:17):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-07-09 13:01:17):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-07-09 13:01:18):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-07-09 13:01:18):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-07-09 13:01:18):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-07-09 13:01:19):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-07-09 13:01:20):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-07-09 13:01:20):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-07-09 13:01:20):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-07-09 13:01:20):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-07-09 13:01:21):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-07-09 13:01:21):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-07-09 13:01:24):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-07-09 13:01:28):Succeed in initializing IS_OPERA.

(2020-07-09 13:02:23):8-O-1Device connected successfully.

(2020-07-09 13:11:08):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-09 13:11:08):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-09 13:11:09):Succeed in initializing IS_OPERA.

(2020-07-13 09:07:32):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-13 09:07:32):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-13 09:07:33):Succeed in initializing IS_OPERA.

(2020-07-14 10:37:44):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-14 10:37:44):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-07-14 10:37:45):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-07-14 10:37:47):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-07-14 10:37:47):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-07-14 10:37:47):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-07-14 10:37:48):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-07-14 10:37:48):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-07-14 10:37:48):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-07-14 10:37:48):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-07-14 10:37:48):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-07-14 10:37:48):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-07-14 10:37:49):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-07-14 10:37:49):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-07-14 10:37:49):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-07-14 10:37:49):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-07-14 10:37:49):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-07-14 10:37:49):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-07-14 10:37:50):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-07-14 10:37:50):Succeed in initializing IS_OPERA.

(2020-07-14 15:58:54):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-14 15:58:54):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-07-15 08:38:28):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-15 08:38:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-15 08:38:29):Succeed in initializing IS_OPERA.

(2020-07-15 14:03:40):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-15 14:03:40):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-15 15:47:36):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-15 15:47:36):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-16 08:44:17):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-16 08:44:17):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-16 08:44:18):Succeed in initializing IS_OPERA.

(2020-07-17 09:18:12):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-17 09:18:12):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-17 09:18:13):Succeed in initializing IS_OPERA.

(2020-07-22 09:59:30):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-22 09:59:30):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-22 09:59:31):Succeed in initializing IS_OPERA.

(2020-07-22 14:05:29):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-22 14:05:29):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-22 14:05:30):Succeed in initializing IS_OPERA.

(2020-07-23 08:43:42):Serial port 8 is not connected to the device.

(2020-07-23 08:43:43):Succeed in initializing IS_OPERA.

(2020-07-24 09:16:58):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-24 09:16:58):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-07-24 09:16:59):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-07-24 09:17:05):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-07-24 09:17:06):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-07-24 09:17:07):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-07-24 09:17:07):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-07-24 09:17:07):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-07-24 09:17:09):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-07-24 09:17:09):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-07-24 09:17:10):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-07-24 09:17:10):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-07-24 09:17:10):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-07-24 09:17:11):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-07-24 09:17:11):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-07-24 09:17:11):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-07-24 09:17:11):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-07-24 09:17:11):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-07-24 09:17:12):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-07-24 09:17:12):Succeed in initializing IS_OPERA.

(2020-07-24 09:18:25):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-24 09:18:25):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-24 09:18:26):Succeed in initializing IS_OPERA.

(2020-07-24 13:00:07):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-24 13:00:07):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-24 13:00:08):Succeed in initializing IS_OPERA.

(2020-07-28 12:01:28):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-28 12:01:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-07-28 12:01:29):Succeed in initializing IS_OPERA.

(2020-07-28 15:50:09):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-07-28 15:50:09):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-11-20 10:47:24):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-11-20 10:47:25):Serial port 2 is not connected to the device.

(2020-11-20 10:47:25):Completing search. No device is connected or serial port is used.

(2020-11-20 10:47:25):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-11-20 10:47:26):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-11-20 10:47:27):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-11-20 10:47:27):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-11-20 10:47:28):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-11-20 10:47:28):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-11-20 10:47:28):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-11-20 10:47:28):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-11-20 10:47:28):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-11-20 10:47:29):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-11-20 10:47:29):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-11-20 10:47:29):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-11-20 10:47:29):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-11-20 10:48:59):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-11-20 10:48:59):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-11-20 10:48:59):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-11-20 10:48:59):Succeed in initializing IS_OPERA.

(2020-11-20 10:49:27):Serial port 2 is not connected to the device.

(2020-11-20 10:49:27):Completing search. No device is connected or serial port is used.

(2020-11-20 10:49:27):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-11-20 10:49:29):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-11-20 10:49:30):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-11-20 10:49:30):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-11-20 10:49:31):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-11-20 10:49:31):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-11-20 10:49:32):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-11-20 10:49:32):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-11-20 10:49:32):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-11-20 10:49:32):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-11-20 10:49:32):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-11-20 10:49:33):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-11-20 10:49:33):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-11-20 10:49:34):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-11-20 10:49:34):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-11-20 10:49:34):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-11-20 10:49:34):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-11-20 10:49:35):Succeed in initializing IS_OPERA.

(2020-11-20 14:21:56):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-11-20 14:21:56):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-11-20 14:21:57):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-11-20 14:21:57):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-11-20 14:21:57):Serial port 2 is not connected to the device.

(2020-11-20 14:21:57):Completing search. No device is connected or serial port is used.

(2020-11-20 14:21:57):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-11-20 14:21:57):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-11-20 14:21:58):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-11-20 14:21:58):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-11-20 14:21:58):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-11-20 14:21:58):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-11-20 14:21:58):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-11-20 14:21:58):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-11-20 14:21:59):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-11-20 14:21:59):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-11-20 14:21:59):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-11-20 14:22:00):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-11-20 14:22:00):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-11-20 14:22:00):Succeed in initializing IS_OPERA.

(2020-11-30 13:49:42):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-11-30 13:49:42):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-11-30 13:49:43):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-11-30 13:49:44):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-11-30 13:49:44):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-11-30 13:49:44):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-11-30 13:49:45):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-11-30 13:49:45):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-11-30 13:49:45):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-11-30 13:49:45):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-11-30 13:49:46):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-11-30 13:49:46):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-11-30 13:49:46):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-11-30 13:49:47):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-11-30 13:49:47):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-11-30 13:49:47):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-11-30 13:49:47):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-11-30 13:49:48):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-11-30 13:49:48):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-11-30 13:49:48):Succeed in initializing IS_OPERA.

(2020-12-01 11:12:22):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-01 11:12:22):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-12-01 11:12:22):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-12-01 11:12:24):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-12-01 11:12:24):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-12-01 11:12:25):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-12-01 11:12:25):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-12-01 11:12:25):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-12-01 11:12:25):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-12-01 11:12:25):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-12-01 11:12:30):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-12-01 11:12:30):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-12-01 11:12:30):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-12-01 11:12:30):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-12-01 11:12:31):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-12-01 11:12:31):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-12-01 11:12:31):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-12-01 11:12:31):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-12-01 11:12:31):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-12-01 11:12:31):Succeed in initializing IS_OPERA.

(2020-12-01 11:13:28):8-O-1Device connected successfully.

(2020-12-01 11:14:15):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-01 11:14:15):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-12-01 11:14:15):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-12-01 11:14:17):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-12-01 11:14:18):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-12-01 11:14:18):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-12-01 11:14:18):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-12-01 11:14:18):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-12-01 11:14:19):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-12-01 11:14:21):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-12-01 11:15:20):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-12-01 11:15:20):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-12-01 11:15:20):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-12-01 11:15:21):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-12-01 11:15:21):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-12-01 11:15:21):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-12-01 11:15:22):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-12-01 11:23:59):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-12-01 11:23:59):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-12-01 11:23:59):Succeed in initializing IS_OPERA.

(2020-12-01 11:49:21):[data exceeding range]:[function code H0536][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0546][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0548][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0552][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0567][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0A41][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0A43][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B07][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B13][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B15][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B17][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B19][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B35][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B53][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B64][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B71][range 0--4194304][running value 0]

(2020-12-01 11:49:21):[data exceeding range]:[function code H0B73][range 0--4194304][running value 0]

(2020-12-01 11:50:03):8-O-1Device connected successfully.

(2020-12-01 11:50:11):[data exceeding range]:[function code H0536][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0546][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0548][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0552][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0567][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0A41][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0A43][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B07][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B13][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B15][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B17][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B19][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B35][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B53][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B64][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B71][range 0--4194304][running value 0]

(2020-12-01 11:50:11):[data exceeding range]:[function code H0B73][range 0--4194304][running value 0]

(2020-12-01 11:54:50):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-01 11:54:50):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-12-01 11:54:50):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-12-01 11:54:52):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-12-01 11:54:52):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-12-01 11:54:53):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-12-01 11:54:53):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-12-01 11:54:53):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-12-01 11:54:53):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-12-01 11:54:53):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-12-01 11:54:54):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-12-01 11:54:54):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-12-01 11:54:54):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-12-01 11:54:54):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-12-01 11:54:54):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-12-01 11:54:55):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-12-01 11:54:55):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-12-01 11:54:55):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-12-01 11:54:55):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-12-01 11:54:55):Succeed in initializing IS_OPERA.

(2020-12-01 11:55:02):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-01 11:55:02):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-01 11:55:04):Succeed in initializing IS_OPERA.

(2020-12-01 13:54:58):Save a recipe file: C:\Users\Patryk\Desktop\20201201135451[IS620P_V].txt

(2020-12-01 13:55:25):Read a recipe file: C:\Users\Patryk\Desktop\20201201135451[IS620P_V].txtInfo.:IS620P_V10.0_E.mdb


(2020-12-01 15:39:27):Save a recipe file: C:\Users\Patryk\Desktop\20201201153925[IS620P_V].txt

(2020-12-03 11:26:54):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-03 11:26:54):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-03 11:26:56):Succeed in initializing IS_OPERA.

(2020-12-03 11:27:04):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-03 11:27:04):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-12-03 11:27:05):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-12-03 11:27:06):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-12-03 11:27:07):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-12-03 11:27:07):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-12-03 11:27:08):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-12-03 11:27:08):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-12-03 11:27:08):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-12-03 11:27:08):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-12-03 11:27:09):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-12-03 11:27:09):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-12-03 11:27:09):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-12-03 11:27:09):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-12-03 11:27:09):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-12-03 11:27:10):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-12-03 11:27:19):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-12-03 11:27:19):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-12-03 11:27:20):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-12-03 11:27:20):Succeed in initializing IS_OPERA.

(2020-12-03 11:27:33):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-03 11:27:33):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-03 11:27:34):Succeed in initializing IS_OPERA.

(2020-12-03 11:28:44):[data exceeding range]:[function code H0208][range 0-0][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0224][range 10-100][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0233][range 0-0][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0381][range 100-800][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0517][range 35-32767][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0524][range 0-1073741824][running value 1153433602]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0552][range 0-2147483647][running value -2063007742]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0554][range 0-127][running value 617152514]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0561][range 0-262143][running value 1426784258]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0618][range 10-6000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0740][range 5-300][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0801][range 15-51200][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0804][range 15-51200][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0823][range 100-4000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0906][range 100-1000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0907][range 20-800][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0908][range 50-10000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0912][range 50-4000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0915][range 50-4000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0918][range 50-4000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0921][range 50-4000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0938][range 10-1000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0942][range 0-2147483647][running value -429981694]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0A04][range 50-300][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0A09][range 100-4000][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0A10][range 1-1073741824][running value -405733374]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0A32][range 10-65535][running value 1]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0B24][range 0-65535][running value 1177026562]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0B55][range -60000-60000][running value 2011234306]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0F04][range 0-1073741824][running value -2032271358]

(2020-12-03 11:28:44):[data exceeding range]:[function code H0F08][range 0-1073741824][running value 1188888578]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1117][range -1073741824-1073741824][running value -1858994174]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1127][range -1073741824-1073741824][running value -1322254334]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1152][range -1073741824-1073741824][running value -2131165182]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1162][range -1073741824-1073741824][running value -1594163198]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1172][range -1073741824-1073741824][running value 1092681730]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1177][range -1073741824-1073741824][running value 1361051650]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1182][range -1073741824-1073741824][running value 1625686018]

(2020-12-03 11:28:44):[data exceeding range]:[function code H1187][range -1073741824-1073741824][running value 1894187010]

(2020-12-03 11:28:44):[data exceeding range]:[function code H3109][range -6000000-6000000][running value 452263938]

(2020-12-03 11:28:44):[data exceeding range]:[function code H3111][range -100000-100000][running value -1154154494]

(2020-12-03 11:44:13):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 11:49:19):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0208][range 0-0][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0224][range 10-100][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0233][range 0-0][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0381][range 100-800][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0517][range 35-32767][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0524][range 0-1073741824][running value 1153433602]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0552][range 0-2147483647][running value -2063007742]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0554][range 0-127][running value 617152514]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0561][range 0-262143][running value 1426784258]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0618][range 10-6000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0740][range 5-300][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0801][range 15-51200][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0804][range 15-51200][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0823][range 100-4000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0906][range 100-1000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0907][range 20-800][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0908][range 50-10000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0912][range 50-4000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0915][range 50-4000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0918][range 50-4000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0921][range 50-4000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0938][range 10-1000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0942][range 0-2147483647][running value -429981694]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0A04][range 50-300][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0A09][range 100-4000][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0A10][range 1-1073741824][running value -405733374]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0A32][range 10-65535][running value 1]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0B24][range 0-65535][running value 1177026562]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0B55][range -60000-60000][running value 2011234306]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0F04][range 0-1073741824][running value -2032271358]

(2020-12-03 11:52:01):[data exceeding range]:[function code H0F08][range 0-1073741824][running value 1188888578]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1117][range -1073741824-1073741824][running value -1858994174]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1127][range -1073741824-1073741824][running value -1322254334]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1152][range -1073741824-1073741824][running value -2131165182]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1162][range -1073741824-1073741824][running value -1594163198]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1172][range -1073741824-1073741824][running value 1092681730]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1177][range -1073741824-1073741824][running value 1361051650]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1182][range -1073741824-1073741824][running value 1625686018]

(2020-12-03 11:52:01):[data exceeding range]:[function code H1187][range -1073741824-1073741824][running value 1894187010]

(2020-12-03 11:52:01):[data exceeding range]:[function code H3109][range -6000000-6000000][running value 452263938]

(2020-12-03 11:52:01):[data exceeding range]:[function code H3111][range -100000-100000][running value -1154154494]

(2020-12-03 11:58:08):[data exceeding range]:[function code H0012][range 10-65535][running value 1]

(2020-12-03 11:58:08):[data exceeding range]:[function code H0013][range 10-65535][running value 1]

(2020-12-03 11:58:08):[data exceeding range]:[function code H0014][range 100-6000][running value 1]

(2020-12-03 11:58:08):[data exceeding range]:[function code H0015][range 100-6000][running value 1]

(2020-12-03 11:58:08):[data exceeding range]:[function code H0017][range 2-360][running value 1]

(2020-12-03 11:58:08):[data exceeding range]:[function code H0031][range 1-1073741824][running value -171114494]

(2020-12-03 11:58:36):[data exceeding range]:[function code H0110][range 2000-20000][running value 1]

(2020-12-03 11:58:36):[data exceeding range]:[function code H0113][range 2-128][running value 1]

(2020-12-03 11:58:36):[data exceeding range]:[function code H0118][range 10-100][running value 1]

(2020-12-03 11:58:36):[data exceeding range]:[function code H0130][range 500-1500][running value 1]

(2020-12-03 11:58:36):[data exceeding range]:[function code H0131][range 100-10000][running value 1]

(2020-12-03 11:58:59):[data exceeding range]:[function code H0208][range 0-0][running value 1]

(2020-12-03 11:58:59):[data exceeding range]:[function code H0224][range 10-100][running value 1]

(2020-12-03 11:58:59):[data exceeding range]:[function code H0233][range 0-0][running value 1]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0517][range 35-32767][running value 1]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0524][range 0-1073741824][running value 1153433602]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0552][range 0-2147483647][running value -2063007742]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0554][range 0-127][running value 617152514]

(2020-12-03 12:06:50):[data exceeding range]:[function code H0561][range 0-262143][running value 1426784258]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0517][range 35-32767][running value 1]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0524][range 0-1073741824][running value 1153433602]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0552][range 0-2147483647][running value -2063007742]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0554][range 0-127][running value 617152514]

(2020-12-03 12:49:23):[data exceeding range]:[function code H0561][range 0-262143][running value 1426784258]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0517][range 35-32767][running value 1]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0524][range 0-1073741824][running value 1153433602]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0552][range 0-2147483647][running value -2063007742]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0554][range 0-127][running value 617152514]

(2020-12-03 12:50:13):[data exceeding range]:[function code H0561][range 0-262143][running value 1426784258]

(2020-12-03 12:50:26):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-03 12:50:26):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-03 12:50:27):Succeed in initializing IS_OPERA.

(2020-12-03 12:50:53):[data exceeding range]:[function code H0208][range 0-0][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0224][range 10-100][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0233][range 0-0][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0381][range 100-800][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0517][range 35-32767][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0524][range 0-1073741824][running value 1153433602]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0552][range 0-2147483647][running value -2063007742]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0554][range 0-127][running value 617152514]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0561][range 0-262143][running value 1426784258]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0618][range 10-6000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0740][range 5-300][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0801][range 15-51200][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0804][range 15-51200][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0823][range 100-4000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0906][range 100-1000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0907][range 20-800][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0908][range 50-10000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0912][range 50-4000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0915][range 50-4000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0918][range 50-4000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0921][range 50-4000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0938][range 10-1000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0942][range 0-2147483647][running value -429981694]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0A04][range 50-300][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0A09][range 100-4000][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0A10][range 1-1073741824][running value -405733374]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0A32][range 10-65535][running value 1]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0B24][range 0-65535][running value 1177026562]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0B55][range -60000-60000][running value 2011234306]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0F04][range 0-1073741824][running value -2032271358]

(2020-12-03 12:50:53):[data exceeding range]:[function code H0F08][range 0-1073741824][running value 1188888578]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1117][range -1073741824-1073741824][running value -1858994174]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1127][range -1073741824-1073741824][running value -1322254334]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1152][range -1073741824-1073741824][running value -2131165182]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1162][range -1073741824-1073741824][running value -1594163198]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1172][range -1073741824-1073741824][running value 1092681730]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1177][range -1073741824-1073741824][running value 1361051650]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1182][range -1073741824-1073741824][running value 1625686018]

(2020-12-03 12:50:53):[data exceeding range]:[function code H1187][range -1073741824-1073741824][running value 1894187010]

(2020-12-03 12:50:53):[data exceeding range]:[function code H3109][range -6000000-6000000][running value 452263938]

(2020-12-03 12:50:53):[data exceeding range]:[function code H3111][range -100000-100000][running value -1154154494]

(2020-12-03 12:51:38):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2020-12-03 12:51:38):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2020-12-03 12:51:38):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2020-12-08 13:44:25):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-08 13:44:25):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-08 13:44:27):Succeed in initializing IS_OPERA.

(2020-12-08 13:44:59):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-08 13:44:59):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-12-08 13:44:59):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-12-08 13:45:13):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-12-08 13:45:14):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-12-08 13:45:14):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-12-08 13:45:14):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-12-08 13:45:15):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-12-08 13:45:15):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-12-08 13:45:15):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-12-08 13:45:15):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-12-08 13:45:15):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-12-08 13:45:15):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-12-08 13:45:16):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-12-08 13:45:16):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-12-08 13:45:16):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-12-08 13:45:17):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-12-08 13:45:17):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-12-08 13:45:18):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-12-08 13:45:18):Succeed in initializing IS_OPERA.

(2020-12-08 13:45:42):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-08 13:45:42):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-08 13:45:43):Succeed in initializing IS_OPERA.

(2020-12-08 13:46:08):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-08 13:46:08):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2020-12-08 13:46:08):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2020-12-08 13:46:10):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2020-12-08 13:46:10):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2020-12-08 13:46:10):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2020-12-08 13:46:11):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2020-12-08 13:46:11):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2020-12-08 13:46:11):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2020-12-08 13:46:11):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2020-12-08 13:46:12):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2020-12-08 13:46:12):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2020-12-08 13:46:12):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2020-12-08 13:46:12):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2020-12-08 13:46:13):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2020-12-08 13:46:13):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2020-12-08 13:46:13):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2020-12-08 13:46:14):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2020-12-08 13:46:14):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2020-12-08 13:46:14):Succeed in initializing IS_OPERA.

(2020-12-08 13:46:53):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-08 13:46:53):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-08 13:46:54):Succeed in initializing IS_OPERA.

(2020-12-08 13:48:03):8-O-1Device connected successfully.

(2020-12-08 13:48:15):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-08 13:48:15):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-08 13:48:16):Succeed in initializing IS_OPERA.

(2020-12-08 13:50:01):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2020-12-08 13:50:01):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2020-12-08 13:50:02):Succeed in initializing IS_OPERA.

(2021-02-02 08:12:52):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-02-02 08:12:52):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-02-02 08:12:54):Succeed in initializing IS_OPERA.

(2021-02-02 11:37:59):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-02-02 11:37:59):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-02-02 11:38:00):Succeed in initializing IS_OPERA.

(2021-02-09 15:44:31):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-02-09 15:44:31):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-02-09 15:44:32):Succeed in initializing IS_OPERA.

(2021-02-09 15:44:50):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-02-09 15:44:50):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-02-09 15:44:51):Succeed in initializing IS_OPERA.

(2021-02-17 10:12:50):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-02-17 10:12:50):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-02-17 10:12:51):Succeed in initializing IS_OPERA.

(2021-02-17 10:13:37):8-O-1Fail to connect device.

(2021-02-17 10:13:38):8-O-1Device connected successfully.

(2021-02-19 10:21:21):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-02-19 10:21:21):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-02-19 10:21:22):Succeed in initializing IS_OPERA.

(2021-03-12 15:10:06):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-03-12 15:10:06):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2021-03-12 15:10:06):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2021-03-12 15:10:07):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2021-03-12 15:10:07):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2021-03-12 15:10:08):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2021-03-12 15:10:08):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2021-03-12 15:10:08):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2021-03-12 15:10:08):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2021-03-12 15:10:08):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2021-03-12 15:10:08):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2021-03-12 15:10:09):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2021-03-12 15:10:09):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2021-03-12 15:10:09):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2021-03-12 15:10:09):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2021-03-12 15:10:09):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2021-03-12 15:10:10):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2021-03-12 15:10:10):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2021-03-12 15:10:10):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2021-03-12 15:10:10):Succeed in initializing IS_OPERA.

(2021-03-12 15:15:40):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-03-12 15:15:40):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2021-03-12 15:15:40):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2021-03-12 15:15:51):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2021-03-12 15:15:51):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2021-03-12 15:15:52):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2021-03-12 15:15:52):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2021-03-12 15:15:52):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2021-03-12 15:15:52):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2021-03-12 15:15:53):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2021-03-12 15:15:53):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2021-03-12 15:15:53):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2021-03-12 15:15:54):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2021-03-12 15:15:54):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2021-03-12 15:15:55):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2021-03-12 15:15:55):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2021-03-12 15:15:56):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2021-03-12 15:15:56):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2021-03-12 15:15:57):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2021-03-12 15:15:57):Succeed in initializing IS_OPERA.

(2021-03-12 15:16:05):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-03-12 15:16:05):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-03-12 15:16:05):Succeed in initializing IS_OPERA.

(2021-03-12 15:16:31):8-O-1Device connected successfully.

(2021-03-12 15:26:41):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-03-12 15:26:41):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-03-12 15:26:43):Succeed in initializing IS_OPERA.

(2021-03-24 10:09:54):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-03-24 10:09:54):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-03-24 10:09:55):Succeed in initializing IS_OPERA.

(2021-03-31 15:52:42):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-03-31 15:52:42):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-03-31 15:52:44):Succeed in initializing IS_OPERA.

(2021-04-06 13:30:43):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-04-06 13:30:43):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-04-06 13:30:44):Succeed in initializing IS_OPERA.

(2021-04-06 13:31:27):[data exceeding range]:[function code H0208][range 0-0][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0224][range 10-100][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0233][range 0-0][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0381][range 100-800][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0502][range 0-1048576][running value 1694957570]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0507][range 1-1073741824][running value 1963327490]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0511][range 1-1073741824][running value -1257963518]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0513][range 1-1073741824][running value 1426325506]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0517][range 35-32767][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0524][range 0-1073741824][running value 1153433602]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0552][range 0-2147483647][running value -2063007742]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0554][range 0-127][running value 617152514]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0561][range 0-262143][running value 1426784258]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0618][range 10-6000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0740][range 5-300][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0801][range 15-51200][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0804][range 15-51200][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0823][range 100-4000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0906][range 100-1000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0907][range 20-800][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0908][range 50-10000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0912][range 50-4000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0915][range 50-4000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0918][range 50-4000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0921][range 50-4000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0938][range 10-1000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0942][range 0-2147483647][running value -429981694]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0A04][range 50-300][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0A09][range 100-4000][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0A10][range 1-1073741824][running value -405733374]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0A32][range 10-65535][running value 1]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0B24][range 0-65535][running value 1177026562]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0B55][range -60000-60000][running value 2011234306]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0F04][range 0-1073741824][running value -2032271358]

(2021-04-06 13:31:27):[data exceeding range]:[function code H0F08][range 0-1073741824][running value 1188888578]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1117][range -1073741824-1073741824][running value -1858994174]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1127][range -1073741824-1073741824][running value -1322254334]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1152][range -1073741824-1073741824][running value -2131165182]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1162][range -1073741824-1073741824][running value -1594163198]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1172][range -1073741824-1073741824][running value 1092681730]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1177][range -1073741824-1073741824][running value 1361051650]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1182][range -1073741824-1073741824][running value 1625686018]

(2021-04-06 13:31:27):[data exceeding range]:[function code H1187][range -1073741824-1073741824][running value 1894187010]

(2021-04-06 13:31:27):[data exceeding range]:[function code H3109][range -6000000-6000000][running value 452263938]

(2021-04-06 13:31:27):[data exceeding range]:[function code H3111][range -100000-100000][running value -1154154494]

(2021-04-06 13:32:47):8-O-1Device connected successfully.

(2021-04-19 12:35:39):Find a servo connection: 1. Serial port No.: COM1
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-04-19 12:35:39):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-04-19 12:35:40):Succeed in initializing IS_OPERA.

(2021-04-19 12:35:58):Software reset succeeds.

(2021-04-19 12:49:30):8-O-1Device connected successfully.

(2021-04-19 12:50:40):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-04-19 12:50:40):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-04-19 12:50:41):Succeed in initializing IS_OPERA.

(2021-04-19 12:50:56):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-04-19 12:50:56):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2021-04-19 12:50:56):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2021-04-19 12:51:00):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2021-04-19 12:51:01):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2021-04-19 12:51:01):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2021-04-19 12:51:02):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2021-04-19 12:51:02):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2021-04-19 12:51:02):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2021-04-19 12:51:03):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2021-04-19 12:51:03):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2021-04-19 12:51:03):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2021-04-19 12:51:04):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2021-04-19 12:51:04):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2021-04-19 12:51:04):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2021-04-19 12:51:05):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2021-04-19 12:51:05):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2021-04-19 12:51:05):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2021-04-19 12:51:06):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2021-04-19 12:51:06):Succeed in initializing IS_OPERA.

(2021-04-19 12:51:26):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-04-19 12:51:26):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-04-19 12:51:26):Succeed in initializing IS_OPERA.

(2021-05-06 13:13:49):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-05-06 13:13:49):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-05-06 13:13:51):Succeed in initializing IS_OPERA.

(2021-05-06 13:36:52):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-05-06 13:36:52):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-05-06 13:36:52):Succeed in initializing IS_OPERA.

(2021-05-21 12:19:51):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-05-21 12:19:51):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-05-21 12:19:52):Succeed in initializing IS_OPERA.

(2021-05-21 12:20:43):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-05-21 12:20:43):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-05-21 12:20:44):Succeed in initializing IS_OPERA.

(2021-06-02 10:32:46):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-06-02 10:32:46):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-06-02 10:32:47):Succeed in initializing IS_OPERA.

(2021-06-02 11:25:16):8-O-1Device connected successfully.

(2021-06-07 12:34:45):Serial port 8 is not connected to the device.

(2021-06-07 12:34:46):Succeed in initializing IS_OPERA.

(2021-06-08 12:14:14):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-06-08 12:14:14):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-06-08 12:14:15):Succeed in initializing IS_OPERA.

(2021-06-10 14:05:18):Serial port 8 is not connected to the device.

(2021-06-10 14:05:18):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-06-10 14:05:18):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-06-10 14:05:20):Succeed in initializing IS_OPERA.

(2021-07-02 10:13:28):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-07-02 10:13:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-07-02 10:13:29):Succeed in initializing IS_OPERA.

(2021-07-02 12:47:16):8-O-1Device connected successfully.

(2021-07-21 08:20:42):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-07-21 08:20:42):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-07-21 08:20:44):Succeed in initializing IS_OPERA.

(2021-07-21 08:25:54):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-07-21 08:25:54):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-07-21 08:25:55):Succeed in initializing IS_OPERA.

(2021-07-23 08:23:40):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-07-23 08:23:40):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-07-23 08:23:41):Succeed in initializing IS_OPERA.

(2021-07-23 08:26:43):[data exceeding range]:[function code H0B01][range -9999-9999][running value 65398]

(2021-07-23 08:26:43):[data exceeding range]:[function code H0B02][range -3000-3000][running value 65491]

(2021-07-23 13:56:13):8-O-1Device connected successfully.

(2021-07-23 14:01:24):8-O-1Device connected successfully.

(2021-07-23 14:56:53):8-O-1Fail to connect device.

(2021-07-23 14:57:08):8-O-1Fail to connect device.

(2021-07-23 14:57:09):8-O-1Device connected successfully.

(2021-07-28 08:21:28):Serial port 8 is not connected to the device.

(2021-07-28 08:21:29):Succeed in initializing IS_OPERA.

(2021-07-28 08:21:47):8-O-1Device connected successfully.

(2021-07-28 08:58:05):Save a recipe file: C:\Users\handlowniec5\Desktop\20210728085755[IS620P_V].txt

(2021-07-28 09:06:53):Save a recipe file: C:\Users\handlowniec5\Desktop\20210728085755[IS620P_V].txt

(2021-07-28 10:43:59):Read a recipe file: C:\Users\handlowniec5\Desktop\20210728085755[IS620P_V].txtInfo.:IS620P_V10.0_E.mdb


(2021-07-29 08:15:10):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-07-29 08:15:10):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-07-29 08:15:11):Succeed in initializing IS_OPERA.

(2021-07-29 10:34:49):8-O-1Device connected successfully.

(2021-07-29 10:35:19):[data exceeding range]:[function code H0200][range 0-6][running value 8]

(2021-07-29 11:02:49):[data exceeding range]:[function code H0200][range 0-6][running value 8]

(2021-07-30 09:20:27):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-07-30 09:20:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-07-30 09:20:28):Succeed in initializing IS_OPERA.

(2021-08-03 08:15:21):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-03 08:15:21):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-03 08:15:22):Succeed in initializing IS_OPERA.

(2021-08-03 09:56:44):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-03 09:56:44):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-03 09:56:45):Succeed in initializing IS_OPERA.

(2021-08-04 08:11:09):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-04 08:11:09):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-04 08:11:10):Succeed in initializing IS_OPERA.

(2021-08-04 10:50:51):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-04 10:50:51):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-04 10:50:51):Succeed in initializing IS_OPERA.

(2021-08-04 10:51:05):[data exceeding range]:[function code H0208][range 0-0][running value 1]

(2021-08-04 10:51:05):[data exceeding range]:[function code H0224][range 10-100][running value 1]

(2021-08-04 10:51:05):[data exceeding range]:[function code H0233][range 0-0][running value 1]

(2021-08-04 10:51:37):8-O-1Device connected successfully.

(2021-08-04 10:51:57):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-04 10:51:57):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-04 10:51:58):Succeed in initializing IS_OPERA.

(2021-08-04 12:24:42):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-04 12:24:42):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-08-04 12:24:43):Succeed in initializing IS_OPERA.

(2021-08-04 12:31:22):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-04 12:31:22):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-04 12:31:22):Succeed in initializing IS_OPERA.

(2021-08-09 09:36:36):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-09 09:36:36):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-09 09:36:37):Succeed in initializing IS_OPERA.

(2021-08-10 08:08:02):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-10 08:08:02):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-10 08:08:03):Succeed in initializing IS_OPERA.

(2021-08-17 14:43:24):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-17 14:43:24):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-17 14:43:24):Succeed in initializing IS_OPERA.

(2021-08-17 14:43:33):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-17 14:43:33):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-08-17 14:43:42):8-O-1Device connected successfully.

(2021-08-18 11:54:26):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-18 11:54:26):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-08-18 11:54:27):Succeed in initializing IS_OPERA.

(2021-08-18 15:01:45):8-O-1Fail to connect device.

(2021-08-18 15:01:47):8-O-1Device connected successfully.

(2021-08-19 08:58:56):Serial port 8 is not connected to the device.

(2021-08-19 08:58:57):Succeed in initializing IS_OPERA.

(2021-08-26 14:18:51):Serial port 8 is not connected to the device.

(2021-08-26 14:18:52):Succeed in initializing IS_OPERA.

(2021-08-31 10:09:30):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-31 10:09:30):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-08-31 10:09:31):Succeed in initializing IS_OPERA.

(2021-08-31 10:12:10):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-31 10:12:10):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-08-31 10:12:11):Succeed in initializing IS_OPERA.

(2021-08-31 10:12:43):8-O-1Device connected successfully.

(2021-08-31 11:35:35):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-08-31 11:35:35):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-08-31 11:35:36):Succeed in initializing IS_OPERA.

(2021-09-20 08:50:19):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-09-20 08:50:19):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-09-20 08:50:21):Succeed in initializing IS_OPERA.

(2021-09-23 09:56:24):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-09-23 09:56:24):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-09-23 09:56:26):Succeed in initializing IS_OPERA.

(2021-09-24 13:16:10):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-09-24 13:16:10):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-09-24 13:16:11):Succeed in initializing IS_OPERA.

(2021-09-27 11:57:02):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-09-27 11:57:02):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-09-27 11:57:03):Succeed in initializing IS_OPERA.

(2021-09-27 11:57:17):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-09-27 11:57:17):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-09-27 11:57:24):8-O-1Device connected successfully.

(2021-09-27 12:00:57):Software reset succeeds.

(2021-09-28 08:14:50):Serial port 8 is not connected to the device.

(2021-09-28 08:14:52):Succeed in initializing IS_OPERA.

(2021-09-28 11:30:33):Serial port 8 is not connected to the device.

(2021-09-28 11:30:33):Succeed in initializing IS_OPERA.

(2021-09-28 13:13:51):Serial port 8 is not connected to the device.

(2021-09-28 13:13:51):Succeed in initializing IS_OPERA.

(2021-10-01 13:47:15):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-01 13:47:15):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-01 13:47:16):Succeed in initializing IS_OPERA.

(2021-10-04 09:23:37):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-04 09:23:37):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-04 09:23:38):Succeed in initializing IS_OPERA.

(2021-10-04 11:49:44):8-O-1Device connected successfully.

(2021-10-04 14:44:40):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-04 14:44:40):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-04 14:44:42):Succeed in initializing IS_OPERA.

(2021-10-04 15:34:21):Serial port 8 is not connected to the device.

(2021-10-04 15:34:22):Succeed in initializing IS_OPERA.

(2021-10-05 10:39:07):Serial port 8 is not connected to the device.

(2021-10-05 10:39:08):Succeed in initializing IS_OPERA.

(2021-10-06 10:11:56):Serial port 8 is not connected to the device.

(2021-10-06 10:11:57):Succeed in initializing IS_OPERA.

(2021-10-06 10:21:33):8-O-1Device connected successfully.

(2021-10-06 10:56:07):Save a recipe file: C:\Users\handlowniec5\Desktop\20211006105317[IS620P_V].txt

(2021-10-06 10:58:00):Read a recipe file: C:\Users\handlowniec5\Desktop\20211006105317[IS620P_V].txtInfo.:IS620P_V10.0_E.mdb


(2021-10-06 11:37:02):Save a recipe file: C:\Users\handlowniec5\Desktop\20211006113659[IS620P_V].txt

(2021-10-06 12:01:28):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-06 12:01:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-06 12:01:29):Succeed in initializing IS_OPERA.

(2021-10-07 09:31:32):Succeed in initializing IS_OPERA.

(2021-10-07 09:31:32):Serial port 8 is not connected to the device.

(2021-10-08 14:09:19):Succeed in initializing IS_OPERA.

(2021-10-08 14:09:19):Serial port 8 is not connected to the device.

(2021-10-13 09:21:29):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-13 09:21:29):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-13 09:21:31):Succeed in initializing IS_OPERA.

(2021-10-18 09:47:10):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-18 09:47:10):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2021-10-18 09:47:11):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2021-10-18 09:47:12):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2021-10-18 09:47:12):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2021-10-18 09:47:12):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2021-10-18 09:47:13):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2021-10-18 09:47:16):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2021-10-18 09:47:18):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2021-10-18 09:47:21):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2021-10-18 09:47:21):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2021-10-18 09:47:21):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2021-10-18 09:47:22):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2021-10-18 09:47:22):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2021-10-18 09:47:22):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2021-10-18 09:47:22):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2021-10-18 09:47:22):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2021-10-18 09:47:22):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2021-10-18 09:47:23):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2021-10-18 09:47:23):Succeed in initializing IS_OPERA.

(2021-10-18 10:10:59):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-18 10:10:59):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-18 10:11:00):Succeed in initializing IS_OPERA.

(2021-10-18 12:35:56):8-O-1Device connected successfully.

(2021-10-18 12:42:52):Database backup file not found.

(2021-10-18 12:42:52):Restore default database file:IS620P_V10.0_E.mdb

(2021-10-18 12:53:27):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-18 12:53:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-18 12:53:43):8-O-1Device connected successfully.

(2021-10-19 08:37:28):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-19 08:37:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-19 08:37:29):Succeed in initializing IS_OPERA.

(2021-10-19 14:22:09):Database backup file not found.

(2021-10-19 14:22:09):Restore default database file:IS620P_V10.0_E.mdb

(2021-10-19 14:52:03):Save a recipe file: C:\Users\handlowniec5\Desktop\20211019145159[IS620P_V].txt

(2021-10-20 08:52:23):Serial port 8 is not connected to the device.

(2021-10-20 08:52:25):Succeed in initializing IS_OPERA.

(2021-10-20 13:45:37):Read a recipe file: C:\Users\handlowniec5\Desktop\20-10-2021.txtInfo.:IS620P_V10.0_E.mdb


(2021-10-20 14:49:57):Read a recipe file: C:\Users\handlowniec5\Desktop\20-10-2021.txtInfo.:IS620P_V10.0_E.mdb


(2021-10-20 15:00:06):Save a recipe file: C:\Users\handlowniec5\Desktop\20211020150000[IS620P_V].txt

(2021-10-21 08:52:20):Succeed in initializing IS_OPERA.

(2021-10-21 08:52:20):Serial port 8 is not connected to the device.

(2021-10-21 09:11:17):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-21 09:11:17):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-22 10:26:50):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-22 10:26:50):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-22 10:26:52):Succeed in initializing IS_OPERA.

(2021-10-25 15:13:25):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-25 15:13:25):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-25 15:13:26):Succeed in initializing IS_OPERA.

(2021-10-26 15:59:07):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-26 15:59:07):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-26 15:59:08):Succeed in initializing IS_OPERA.

(2021-10-27 10:26:33):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-10-27 10:26:33):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-10-27 10:26:34):Succeed in initializing IS_OPERA.

(2021-10-27 10:26:51):8-O-1Device connected successfully.

(2021-10-27 14:07:24):Serial port 8 is not connected to the device.

(2021-10-27 14:07:24):Succeed in initializing IS_OPERA.

(2021-10-27 15:51:06):8-O-1Device connected successfully.

(2021-10-28 09:23:43):Serial port 8 is not connected to the device.

(2021-10-28 09:23:44):Succeed in initializing IS_OPERA.

(2021-10-28 13:45:28):8-O-1Fail to connect device.

(2021-10-29 14:28:00):Succeed in initializing IS_OPERA.

(2021-10-29 14:28:01):Serial port 8 is not connected to the device.

(2021-10-29 15:25:34):Read a recipe file: C:\Users\handlowniec5\Desktop\20211029150555[IS620P_C].txtInfo.:IS620P_CANopenV2.1_E.mdb

(2021-10-29 15:25:34):[exceeding range]:[function code H0B21][range -1200-1200][current value 65534]

(2021-10-29 15:25:38):[exceeding range]:[function code H0B22][range -1200-1200][current value 65534]

(2021-11-02 09:16:39):Succeed in initializing IS_OPERA.

(2021-11-02 09:16:40):Serial port 8 is not connected to the device.

(2021-11-04 11:38:37):Succeed in initializing IS_OPERA.

(2021-11-04 11:38:37):Serial port 8 is not connected to the device.

(2021-11-09 12:21:18):Succeed in initializing IS_OPERA.

(2021-11-09 12:21:19):Serial port 8 is not connected to the device.

(2021-11-19 12:09:59):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-11-19 12:09:59):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-11-19 12:10:00):Succeed in initializing IS_OPERA.

(2021-11-19 12:17:33):8-O-1Device connected successfully.

(2021-11-19 15:40:31):Succeed in initializing IS_OPERA.

(2021-11-19 15:40:32):Serial port 8 is not connected to the device.

(2021-11-23 12:03:58):Succeed in initializing IS_OPERA.

(2021-11-23 12:03:59):Serial port 8 is not connected to the device.

(2021-11-25 14:46:41):Serial port 8 is not connected to the device.

(2021-11-25 14:46:42):Succeed in initializing IS_OPERA.

(2021-11-26 11:42:31):Serial port 8 is not connected to the device.

(2021-11-26 11:42:31):Succeed in initializing IS_OPERA.

(2021-11-30 08:24:48):Serial port 8 is not connected to the device.

(2021-11-30 08:24:48):Succeed in initializing IS_OPERA.

(2021-12-02 09:40:16):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-02 09:40:16):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-02 09:40:17):Succeed in initializing IS_OPERA.

(2021-12-02 11:02:56):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-02 11:02:56):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-02 11:02:57):Succeed in initializing IS_OPERA.

(2021-12-02 11:15:46):8-O-1Device connected successfully.

(2021-12-02 11:16:09):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-02 11:16:10):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-12-02 11:16:10):Succeed in initializing IS_OPERA.

(2021-12-02 11:34:26):8-O-1Device connected successfully.

(2021-12-02 11:35:47):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65535]

(2021-12-02 12:40:41):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-02 12:40:41):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-02 12:40:42):Succeed in initializing IS_OPERA.

(2021-12-06 08:36:32):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-06 08:36:32):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2021-12-06 08:36:33):Succeed in initializing IS_OPERA.

(2021-12-06 08:36:49):8-O-1Device connected successfully.

(2021-12-06 13:51:33):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-06 13:51:33):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-06 13:51:35):Succeed in initializing IS_OPERA.

(2021-12-07 08:15:01):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-07 08:15:01):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-07 08:15:03):Succeed in initializing IS_OPERA.

(2021-12-07 08:23:25):8-O-1Device connected successfully.

(2021-12-07 08:26:12):8-O-1Device connected successfully.

(2021-12-07 10:42:58):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-07 10:42:58):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-07 11:55:52):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-07 11:55:52):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-07 11:55:53):Succeed in initializing IS_OPERA.

(2021-12-07 14:45:30):8-O-1Device connected successfully.

(2021-12-07 14:48:34):Software reset fails
Error code: 00000004.

(2021-12-08 13:12:28):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-08 13:12:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-08 13:12:30):Succeed in initializing IS_OPERA.

(2021-12-08 13:12:53):8-O-1Fail to connect device.

(2021-12-08 13:13:06):8-N-2Fail to connect device.

(2021-12-08 13:13:23):8-N-1Fail to connect device.

(2021-12-08 13:14:40):8-N-2Fail to connect device.

(2021-12-08 13:15:35):8-N-2Fail to connect device.

(2021-12-08 13:21:25):8-N-2Device connected successfully.

(2021-12-08 13:21:59):8-N-2Device connected successfully.

(2021-12-08 13:23:17):8-N-2Device connected successfully.

(2021-12-08 14:15:17):8-N-2Fail to connect device.

(2021-12-08 14:15:35):8-N-1Fail to connect device.

(2021-12-08 14:17:52):8-N-2Device connected successfully.

(2021-12-09 11:39:28):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-09 11:39:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-09 11:39:29):Succeed in initializing IS_OPERA.

(2021-12-09 11:40:41):[data exceeding range]:[function code H0208][range 0-0][running value 1]

(2021-12-09 11:40:41):[data exceeding range]:[function code H0224][range 10-100][running value 1]

(2021-12-09 11:40:41):[data exceeding range]:[function code H0233][range 0-0][running value 1]

(2021-12-09 11:42:14):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-09 11:42:14):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-09 11:42:15):Succeed in initializing IS_OPERA.

(2021-12-09 12:26:44):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-09 12:26:44):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-09 12:26:45):Succeed in initializing IS_OPERA.

(2021-12-10 09:51:50):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-10 09:51:50):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-10 09:51:51):Succeed in initializing IS_OPERA.

(2021-12-10 09:52:22):8-N-2Fail to connect device.

(2021-12-10 09:52:43):8-N-2Device connected successfully.

(2021-12-10 09:56:41):8-N-2Device connected successfully.

(2021-12-10 11:54:40):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-10 11:54:40):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-10 11:54:41):Succeed in initializing IS_OPERA.

(2021-12-13 08:45:53):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-13 08:45:53):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-13 08:45:55):Succeed in initializing IS_OPERA.

(2021-12-14 09:43:55):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-14 09:43:55):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-14 09:43:57):Succeed in initializing IS_OPERA.

(2021-12-15 08:31:07):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-15 08:31:07):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-15 08:31:08):Succeed in initializing IS_OPERA.

(2021-12-16 13:12:20):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-16 13:12:20):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-16 13:12:21):Succeed in initializing IS_OPERA.

(2021-12-17 13:32:40):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-17 13:32:40):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-17 13:32:41):Succeed in initializing IS_OPERA.

(2021-12-20 09:48:52):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-20 09:48:52):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-20 09:48:53):Succeed in initializing IS_OPERA.

(2021-12-21 08:40:12):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-21 08:40:12):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-21 08:40:13):Succeed in initializing IS_OPERA.

(2021-12-21 10:06:31):8-N-2Device connected successfully.

(2021-12-21 10:08:49):Software reset fails
Error code: 00000004.

(2021-12-21 10:20:11):Find a servo connection: 1. Serial port No.: COM14
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-21 10:20:11):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-23 09:54:22):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2021-12-23 09:54:22):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2021-12-23 09:54:23):Succeed in initializing IS_OPERA.

(2022-01-03 08:11:22):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-03 08:11:22):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-01-03 08:11:23):Succeed in initializing IS_OPERA.

(2022-01-04 08:56:17):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-04 08:56:17):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-01-04 08:56:19):Succeed in initializing IS_OPERA.

(2022-01-12 09:36:28):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-12 09:36:28):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-01-12 09:36:29):Succeed in initializing IS_OPERA.

(2022-01-13 08:08:00):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-13 08:08:00):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-01-13 08:08:02):Succeed in initializing IS_OPERA.

(2022-01-21 08:41:25):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-21 08:41:25):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-01-21 08:41:27):Succeed in initializing IS_OPERA.

(2022-01-25 11:51:10):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :9600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-25 11:51:10):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-01-25 11:51:12):Succeed in initializing IS_OPERA.

(2022-01-25 12:28:33):8-N-2Fail to connect device.

(2022-01-25 12:28:45):8-N-1Fail to connect device.

(2022-01-25 12:28:56):8-N-2Fail to connect device.

(2022-01-25 12:32:52):8-N-2Fail to connect device.

(2022-01-25 12:34:36):Serial port 8 is not connected to the device.

(2022-01-25 12:34:36):Succeed in initializing IS_OPERA.

(2022-01-25 12:34:52):8-N-2Fail to connect device.

(2022-01-25 12:35:26):8-N-2Device connected successfully.

(2022-01-25 12:55:23):Software reset succeeds.

(2022-01-26 09:55:45):Succeed in initializing IS_OPERA.

(2022-01-26 09:55:45):Serial port 8 is not connected to the device.

(2022-01-26 10:45:27):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-26 10:45:27):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2022-01-26 10:45:27):Succeed in initializing IS_OPERA.

(2022-01-26 10:45:38):8-N-2Device connected successfully.

(2022-01-26 10:46:09):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2022-01-26 11:09:30):Software reset succeeds.

(2022-01-26 11:10:12):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65533]

(2022-01-26 11:13:14):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65533]

(2022-01-26 11:26:15):[data exceeding range]:[function code H0C14][range 1-4][running value 0]

(2022-01-26 13:19:22):Succeed in copying file:C:\Users\handlowniec5\Desktop\INOVANCE\Serwo\InoServoShop_V4.10.0.30_20200104\data\IS620CO do nawijania na bebenmdb.mdb

(2022-01-27 08:42:55):Succeed in initializing IS_OPERA.

(2022-01-27 08:42:56):Serial port 8 is not connected to the device.

(2022-01-28 11:54:20):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-01-28 11:54:20):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2022-01-28 11:54:21):Succeed in initializing IS_OPERA.

(2022-01-28 11:54:43):Find a servo connection: 1. Serial port No.: COM8
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is  during parameter download.

(2022-01-28 11:54:43):Current software version of the servo:  0000010e, database: IS620P_CANopenV2.1_E.mdb

(2022-01-28 11:54:55):8-N-2Device connected successfully.

(2022-02-08 11:03:53):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-02-08 11:03:53):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-02-08 11:03:54):Succeed in initializing IS_OPERA.

(2022-02-09 09:59:32):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-02-09 09:59:32):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-02-09 09:59:33):Succeed in initializing IS_OPERA.

(2022-02-10 09:31:26):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-02-10 09:31:26):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-02-10 09:31:27):Succeed in initializing IS_OPERA.

(2022-03-07 11:42:58):Succeed in initializing IS_OPERA.

(2022-03-07 11:42:59):Serial port 14 is not connected to the device.

(2022-03-07 11:46:22):Succeed in initializing IS_OPERA.

(2022-03-07 11:46:22):Serial port 14 is not connected to the device.

(2022-03-07 11:50:42):8-N-2Fail to connect device.

(2022-03-07 11:52:52):8-N-2Device connected successfully.

(2022-03-07 12:29:10):8-N-2Fail to connect device.

(2022-03-07 12:29:14):COM21 serial port is being used.

(2022-03-07 15:41:36):Succeed in initializing IS_OPERA.

(2022-03-07 15:41:37):Serial port 14 is not connected to the device.

(2022-03-07 16:04:47):Succeed in initializing IS_OPERA.

(2022-03-07 16:04:48):Serial port 14 is not connected to the device.

(2022-03-08 09:08:00):Succeed in initializing IS_OPERA.

(2022-03-08 09:08:01):Serial port 14 is not connected to the device.

(2022-03-08 11:11:10):Serial port 14 is not connected to the device.

(2022-03-08 11:11:10):Succeed in initializing IS_OPERA.

(2022-03-08 12:07:20):Succeed in initializing IS_OPERA.

(2022-03-08 12:07:21):Serial port 14 is not connected to the device.

(2022-03-09 08:10:41):Succeed in initializing IS_OPERA.

(2022-03-09 08:10:42):Serial port 14 is not connected to the device.

(2022-03-09 09:27:16):Succeed in initializing IS_OPERA.

(2022-03-09 09:27:16):Serial port 14 is not connected to the device.

(2022-03-09 09:27:24):8-N-2Device connected successfully.

(2022-03-09 09:27:58):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2022-03-09 09:32:38):Save a recipe file: C:\Users\Patryk.ELDAR\AppData\Roaming\Microsoft\Windows\Network Shortcuts\20220309093233[IS620P_C].txt

(2022-03-09 09:32:45):Save a recipe file: C:\Users\Patryk.ELDAR\AppData\Roaming\Microsoft\Windows\Network Shortcuts\20220309093241[IS620P_C].txt

(2022-03-09 09:34:05):Save a recipe file: C:\Users\Patryk.ELDAR\Desktop\20220309093241[IS620P_C].txt

(2022-03-09 09:34:13):Save a recipe file: C:\Users\Patryk.ELDAR\Desktop\20220309093233[IS620P_C].txt

(2022-03-09 11:15:24):Serial port 8 is not connected to the device.

(2022-03-09 11:15:25):Succeed in initializing IS_OPERA.

(2022-03-10 08:23:44):Serial port 8 is not connected to the device.

(2022-03-10 08:23:45):Succeed in initializing IS_OPERA.

(2022-03-11 09:37:26):Serial port 8 is not connected to the device.

(2022-03-11 09:37:26):Succeed in initializing IS_OPERA.

(2022-03-15 09:30:42):Serial port 8 is not connected to the device.

(2022-03-15 09:30:43):Succeed in initializing IS_OPERA.

(2022-03-17 11:44:22):Succeed in initializing IS_OPERA.

(2022-03-17 11:44:22):Serial port 8 is not connected to the device.

(2022-03-18 10:28:32):Succeed in initializing IS_OPERA.

(2022-03-18 10:28:33):Serial port 8 is not connected to the device.

(2022-03-18 10:33:00):8-N-2Fail to connect device.

(2022-03-18 10:33:04):8-N-2Device connected successfully.

(2022-03-18 10:33:26):8-N-2Device connected successfully.

(2022-03-18 13:16:46):Succeed in initializing IS_OPERA.

(2022-03-18 13:16:47):Serial port 8 is not connected to the device.

(2022-03-22 12:33:16):Succeed in initializing IS_OPERA.

(2022-03-22 12:33:17):Serial port 8 is not connected to the device.

(2022-03-29 13:48:15):Succeed in initializing IS_OPERA.

(2022-03-29 13:48:16):Serial port 8 is not connected to the device.

(2022-03-30 09:27:18):Succeed in initializing IS_OPERA.

(2022-03-30 09:27:18):Serial port 8 is not connected to the device.

(2022-03-31 09:42:23):Serial port 8 is not connected to the device.

(2022-03-31 09:42:24):Succeed in initializing IS_OPERA.

(2022-04-01 11:41:13):Succeed in initializing IS_OPERA.

(2022-04-01 11:41:13):Serial port 8 is not connected to the device.

(2022-04-04 13:02:33):Succeed in initializing IS_OPERA.

(2022-04-04 13:02:33):Serial port 8 is not connected to the device.

(2022-04-05 14:00:04):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-05 14:00:04):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-05 14:00:05):Succeed in initializing IS_OPERA.

(2022-04-11 11:22:14):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-11 11:22:14):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-11 11:22:15):Succeed in initializing IS_OPERA.

(2022-04-13 09:50:17):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-13 09:50:17):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-13 09:50:19):Succeed in initializing IS_OPERA.

(2022-04-14 08:14:36):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-14 08:14:36):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-14 08:14:37):Succeed in initializing IS_OPERA.

(2022-04-19 12:14:53):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-19 12:14:53):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-19 12:14:55):Succeed in initializing IS_OPERA.

(2022-04-20 09:34:09):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-20 09:34:09):Current software version of the servo:  00000001, database: IS620P_AutoTun_V1.3_E.mdb

(2022-04-20 09:34:10):[exceeding range]:[function code H0536][range 0--4194304][current value 0]

(2022-04-20 09:34:11):[exceeding range]:[function code H0546][range 0--4194304][current value 0]

(2022-04-20 09:34:12):[exceeding range]:[function code H0548][range 0--4194304][current value 0]

(2022-04-20 09:34:13):[exceeding range]:[function code H0552][range 0--4194304][current value 0]

(2022-04-20 09:34:13):[exceeding range]:[function code H0567][range 0--4194304][current value 0]

(2022-04-20 09:34:13):[exceeding range]:[function code H0A41][range 0--4194304][current value -4194304]

(2022-04-20 09:34:14):[exceeding range]:[function code H0A43][range 0--4194304][current value 0]

(2022-04-20 09:34:14):[exceeding range]:[function code H0B07][range 0--4194304][current value 0]

(2022-04-20 09:34:14):[exceeding range]:[function code H0B13][range 0--4194304][current value 0]

(2022-04-20 09:34:14):[exceeding range]:[function code H0B15][range 0--4194304][current value 0]

(2022-04-20 09:34:14):[exceeding range]:[function code H0B17][range 0--4194304][current value 0]

(2022-04-20 09:34:15):[exceeding range]:[function code H0B19][range 0--4194304][current value 0]

(2022-04-20 09:34:15):[exceeding range]:[function code H0B35][range 0--4194304][current value 0]

(2022-04-20 09:34:15):[exceeding range]:[function code H0B53][range 0--4194304][current value 0]

(2022-04-20 09:34:15):[exceeding range]:[function code H0B64][range 0--4194304][current value 0]

(2022-04-20 09:34:16):[exceeding range]:[function code H0B71][range 0--4194304][current value 0]

(2022-04-20 09:34:16):[exceeding range]:[function code H0B73][range 0--4194304][current value 0]

(2022-04-20 09:34:16):Succeed in initializing IS_OPERA.

(2022-04-20 09:34:25):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-20 09:34:25):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-20 09:34:26):Succeed in initializing IS_OPERA.

(2022-04-26 12:08:05):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-26 12:08:05):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-26 12:08:06):Succeed in initializing IS_OPERA.

(2022-04-27 11:08:43):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-04-27 11:08:43):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-04-27 11:08:44):Succeed in initializing IS_OPERA.

(2022-05-05 08:34:18):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-05 08:34:18):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-05-05 08:34:23):Succeed in initializing IS_OPERA.

(2022-05-18 11:11:36):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-18 11:11:36):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-05-18 11:11:38):Succeed in initializing IS_OPERA.

(2022-05-19 15:28:04):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-19 15:28:04):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-05-19 15:28:05):Succeed in initializing IS_OPERA.

(2022-05-20 09:33:27):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-20 09:33:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-05-20 09:33:28):Succeed in initializing IS_OPERA.

(2022-05-20 09:34:00):8-N-2Device connected successfully.

(2022-05-20 15:21:47):8-N-2Fail to connect device.

(2022-05-20 15:21:56):8-N-2Fail to connect device.

(2022-05-23 10:12:16):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-23 10:12:16):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-05-23 10:12:17):Succeed in initializing IS_OPERA.

(2022-05-23 10:35:34):8-N-2Device connected successfully.

(2022-05-23 10:36:44):Find a servo connection: 1. Serial port No.: COM19
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-23 10:36:44):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2022-05-23 10:36:45):Succeed in initializing IS_OPERA.

(2022-05-23 10:37:35):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65533]

(2022-05-23 10:52:04):Find a servo connection: 1. Serial port No.: COM19
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-23 10:52:04):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-05-23 10:52:05):Succeed in initializing IS_OPERA.

(2022-05-24 09:03:52):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-05-24 09:03:52):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-05-24 09:03:53):Succeed in initializing IS_OPERA.

(2022-06-01 14:57:27):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-01 14:57:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-01 14:57:28):Succeed in initializing IS_OPERA.

(2022-06-02 15:19:05):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-02 15:19:05):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-02 15:19:06):Succeed in initializing IS_OPERA.

(2022-06-03 09:09:11):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-03 09:09:11):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-03 09:09:12):Succeed in initializing IS_OPERA.

(2022-06-06 10:28:06):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-06 10:28:06):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-06 10:28:07):Succeed in initializing IS_OPERA.

(2022-06-06 11:04:54):8-N-2Device connected successfully.

(2022-06-06 13:13:40):Save a recipe file: C:\Users\Patryk.ELDAR\Desktop\IS620_TEST_VDI.txt

(2022-06-07 08:05:27):Serial port 19 is not connected to the device.

(2022-06-07 08:05:27):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-07 08:05:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-07 08:05:28):Succeed in initializing IS_OPERA.

(2022-06-07 14:32:52):Read a recipe file: C:\Users\Patryk.ELDAR\Desktop\2022-06-07 winda_003.txtInfo.:IS620P_V10.0_E.mdb


(2022-06-07 14:32:52):[exceeding range]:[function code H0B02][range -3000-3000][current value 65507]

(2022-06-07 14:37:50):8-N-2Fail to connect device.

(2022-06-07 14:38:07):8-N-2Fail to connect device.

(2022-06-07 14:38:20):8-N-2Fail to connect device.

(2022-06-07 14:38:56):8-N-2Fail to connect device.

(2022-06-07 14:39:16):8-N-2Device connected successfully.

(2022-06-07 14:41:59):Read a recipe file: C:\Users\Patryk.ELDAR\Desktop\2022-06-07 winda_003.txtInfo.:IS620P_V10.0_E.mdb


(2022-06-07 14:41:59):[exceeding range]:[function code H0B02][range -3000-3000][current value 65507]

(2022-06-07 14:54:03):Read a recipe file: C:\Users\Patryk.ELDAR\Desktop\2022-06-07 winda_003.txtInfo.:IS620P_V10.0_E.mdb


(2022-06-07 14:54:03):[exceeding range]:[function code H0B02][range -3000-3000][current value 65507]

(2022-06-08 08:32:43):Serial port 19 is not connected to the device.

(2022-06-08 08:32:43):Succeed in initializing IS_OPERA.

(2022-06-08 08:39:10):8-N-2Device connected successfully.

(2022-06-09 08:53:03):Serial port 19 is not connected to the device.

(2022-06-09 08:53:05):Succeed in initializing IS_OPERA.

(2022-06-10 15:23:57):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :19200
3. Device ID: 10
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-10 15:23:57):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-10 15:23:58):Succeed in initializing IS_OPERA.

(2022-06-13 11:55:20):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :19200
3. Device ID: 10
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-13 11:55:20):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-13 11:55:21):Succeed in initializing IS_OPERA.

(2022-06-14 15:38:09):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :19200
3. Device ID: 10
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-14 15:38:09):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-14 15:38:10):Succeed in initializing IS_OPERA.

(2022-06-15 09:35:11):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :19200
3. Device ID: 10
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-15 09:35:11):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-15 09:35:12):Succeed in initializing IS_OPERA.

(2022-06-15 10:15:09):8-N-2Fail to connect device.

(2022-06-15 10:15:18):8-N-2Fail to connect device.

(2022-06-15 10:16:37):8-N-2Device connected successfully.

(2022-06-20 14:44:27):Find a servo connection: 1. Serial port No.: COM19
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-20 14:44:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-20 14:44:28):Succeed in initializing IS_OPERA.

(2022-06-21 08:41:50):Serial port 19 is not connected to the device.

(2022-06-21 08:41:51):Succeed in initializing IS_OPERA.

(2022-06-22 08:12:23):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-22 08:12:23):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-22 08:12:24):Succeed in initializing IS_OPERA.

(2022-06-23 09:27:48):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-23 09:27:48):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-23 09:27:49):Succeed in initializing IS_OPERA.

(2022-06-24 09:22:32):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-24 09:22:32):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-24 09:22:33):Succeed in initializing IS_OPERA.

(2022-06-24 09:43:50):8-N-2Device connected successfully.

(2022-06-24 09:45:11):[data exceeding range]:[function code H0200][range 0-6][running value 8]

(2022-06-24 09:48:05):Find a servo connection: 1. Serial port No.: COM19
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-24 09:48:05):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2022-06-24 09:48:05):Succeed in initializing IS_OPERA.

(2022-06-24 10:19:41):[data exceeding range]:[function code H0C14][range 1-4][running value 0]

(2022-06-24 13:50:30):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-24 13:50:30):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2022-06-24 13:50:30):Succeed in initializing IS_OPERA.

(2022-06-27 09:44:57):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-27 09:44:57):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-27 09:44:59):Succeed in initializing IS_OPERA.

(2022-06-30 12:45:24):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-06-30 12:45:24):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-06-30 12:45:26):Succeed in initializing IS_OPERA.

(2022-07-04 08:30:26):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-07-04 08:30:26):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-07-04 08:30:27):Succeed in initializing IS_OPERA.

(2022-07-05 08:43:16):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-07-05 08:43:16):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-07-05 08:43:17):Succeed in initializing IS_OPERA.

(2022-07-06 10:52:51):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2022-07-06 10:52:51):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2022-07-06 10:52:52):Succeed in initializing IS_OPERA.

